!Configurações ASA:

enable

conf t

!Interfece OUTSIDE:

interface gig 0/0

nameif outside

no shutdown

ip address dhcp

exit

!Interfece INSIDE:

interface gig 0/1

nameif inside

no shutdown

ip address 192.168.10.1 255.255.255.0

exit

!DHCP:

dhcpd address 192.168.10.10-192.168.10.100 inside

dhcpd dns 8.8.8.8 interface inside

dhcpd enable inside

!Interface de Gerenciamento

interface management 0/0

ip address 192.168.1.1 255.255.255.0

nameif management

no shutdown

exit

!DHCP

dhcpd address 192.168.1.10-192.168.1.20 management

dhcpd dns 8.8.8.8 interface management

dhcpd enable management

!Configuração WEB

http server enable

http 192.168.1.0 255.255.255.0 management

http 192.168.10.0 255.255.255.0 inside

!Criar usuario Administrador

username admin password senai privilege 15

!ACL

access-list outside\_access\_in extended permit ip any any

access-list inside\_access\_in extended permit ip any any

access-group outside\_access\_in in interface outside

access-group inside\_access\_in in interface inside

!ou para liberar tudo de uma vez utilizar os dois comandos abaixo

!access-list global\_access extended permit ip any any

!access-group global\_access global

!NAT

object network INSIDE

subnet 192.168.10.0 255.255.255.0

nat (INSIDE,OUTSIDE) dynamic interface

exit